Must

Be powered by a wall adaptor 12V

Have an LCD for user feedback

Must have a unique code to unlock

Use an NES controller for user input

- Use 8-2-3 decoder- This will allow us to use less GPIO pins to interface with MCU.

Should

User programmable combination

May

Different ways to unlock

Puzzle game

Back up battery